**

Info Sheet:
Edirol R-09 Audio Recorder
Installing Batteries and Memory Card

Info Sheet:
Edirol R-09 Audio Recorder

Installing Batteries and Memory Card

1. To install batteries, push the flap down while holding the switch left on the bottom of the recorder.
2. The flap should then open. The inside of the flap shows which way to put in a pair of AA batteries.
3. Push the flap down and click it shut.
4. To install a memory card, push the bottom flap downward until it is halfway there. This time, do not push the middle switch.
5. Push the memory card face up into the thin slot on the left.
6. Close the flap.
7. To install batteries, push the flap down while holding the switch left on the bottom of the recorder.
8. The flap should then open. The inside of the flap shows which way to put in a pair of AA batteries.
9. Push the flap down and click it shut.
10. To install a memory card, push the bottom flap downward until it is halfway there. This time, do not push the middle switch.
11. Push the memory card face up into the thin slot on the left.
12. Close the flap.

**

Info Sheet:
Edirol R-09 Audio Recorder
Installing Batteries and Memory Card

Info Sheet:
Edirol R-09 Audio Recorder
Installing Batteries and Memory Card

## More Information

For access to additional information, tutorials and workshops, please visit the Center for Academic Technology website, <http://www.butler.edu/it/cat>, contact any Center for Academic Technology staff member at training@butler.edu,or contact the Information Commons desk in Irwin Library at infocommons@butler.edu or 940-9235.

## More Information

For access to additional information, tutorials and workshops, please visit the Center for Academic Technology website, <http://www.butler.edu/it/cat>, contact any Center for Academic Technology staff member at training@butler.edu,or contact the Information Commons desk in Irwin Library at infocommons@butler.edu or 940-9235.

1. To install batteries, push the flap down while holding the switch left on the bottom of the recorder.
2. The flap should then open. The inside of the flap shows which way to put in a pair of AA batteries.
3. Push the flap down and click it shut.
4. To install a memory card, push the bottom flap downward until it is halfway there. This time, do not push the middle switch.
5. Push the memory card face up into the thin slot on the left.
6. Close the flap.
7. To install batteries, push the flap down while holding the switch left on the bottom of the recorder.
8. The flap should then open. The inside of the flap shows which way to put in a pair of AA batteries.
9. Push the flap down and click it shut.
10. To install a memory card, push the bottom flap downward until it is halfway there. This time, do not push the middle switch.
11. Push the memory card face up into the thin slot on the left.
12. Close the flap.

## More Information

For access to additional information, tutorials and workshops, please visit the Center for Academic Technology website, <http://www.butler.edu/it/cat>, contact any Center for Academic Technology staff member at training@butler.edu,or contact the Information Commons desk in Irwin Library at infocommons@butler.edu or 940-9235.

## More Information

For access to additional information, tutorials and workshops, please visit the Center for Academic Technology website, <http://www.butler.edu/it/cat>, contact any Center for Academic Technology staff member at training@butler.edu,or contact the Information Commons desk in Irwin Library at infocommons@butler.edu or 940-9235.